EXAMPLES OF PART WRITE UPS IN UNIFORM FOR MEMORY

BE DON’T USE “ WE USE IN

BOLT, HEX, 2 IN DIA X 6 5/8 IN LG

BOLT, TYPE OF BOLT, DIA OF BOLT X LENGH OF BOLT AND THREAD PER IN

ACTUATOR, ROTARY, WITH BUTTERFLY VALVE

MOTOR, 440V, 92A, 56.5KW, 60HZ, IP 54, 3565 RPM

MOTOR, 200-230V, 50/ 60HZ, 1/2 HP, TYPE P

MOTOR, ELECTRIC, 230/460V, 48/24A, PH3, 15KW, 60HZ, RPM 1760

BEARING, BLOCK, CAMSHAFT BEARING ON FLYWHEEL END

O RING, 14MM OD X 10MM ID X 3MM THK

O RING, 15 IN OD X 14 IN ID X 8/16 IN THK

O RING, RUBBER, 125MM ID X 120MM OD X 3MM THK

ELEMENT, FILTER, W GASKET KIT

BUSHING, BEARING, 1 7/8 IN OD X 1 1/2 IN ID

BEARING, BALL, 1 7/ 8 IN OD X 7/ 8 IN ID

O RING, OIL PUMP CASING, FORCED

COUPLING, HALF, 82MM, USED, FOR EXHAUST GAS BOILER WATER CIRCULATION PUMP FORWARD

IMPELLER, RAW WATER PUMP, CLOCKWISE TURNING ENGINE, RAW WATER PUMP II

TRANSFORMER, PRI 1-2, 400V, 0.50/ 057 KVA, 50/ 60 HZ, SEC 31-32, 230V, 2.2A

CIRCUIT BREAKER, 10A, 400V, 2 POLE

CIRCUIT BREAKER, 15A, 120/ 240 VOLTS, 2 POLE

BUTTON, PUSH, GREEN

BUTTON, PUSH, RED

BUTTON, PUSH, BLACK

BULB, LED, 24V AC/ DC

BULB, 28V, 40MA

BREAKER, 3-POLE, 20 AMP, 240VAC TYPE THQL

ACTUATOR, DOUBLE ACTION, PRESSURE 125

ACTUATOR, PNEUMATIC

ACTUATOR, GOVERNOR, EMERGENCY DIESEL

PLATE, LOCKING, 83MM LG X 17MM W X 1MM THK, WITH 2 OVAL HOLES 10MM X 8MM

AMPS ARE MORE IMPORTANT FOR ELECTRICAL COMPONENTS SO IT WOULD COME FIRST EXAMPLE AMPS, VOLTS, WATTS, HERTZ, PHASE

NORMAL SPARE PARTS GO IN ORDER OF VOLTS, AMPS, WATTS, HERTZ, PHASE, IP OR ENCLOSER, RPM, AND SO ON

WE ABBRIVATE THEM SO IT WOULD BE AS EXAMPLE 220V, 80A, 100W, 50/ 60HZ, 3 PHASE